Merge Board

* + Current controlled positive high voltage ideal diode controller (Current merge circuit) to get a 200A output from two 100A batteries at 14.8V.
  + 14.8V, 140A output for motors through kill switch to turn off the motors for safety.
  + Current sensing using current shunt monitors and Arduino microcontroller.

