Material Safety Data Sheet

<http://www.nrel.gov/education/pdfs/lithium-ion_battery_materials_safety_data_sheet.pdf>

Minimum safe voltage 12V

Maximum safe voltage 16.8V

Charging 90% Voltage 15.12V

Charging 95% Voltage 15.96V

Maximum continuous Current Draw per Battery 100Amps