Backplane

* + Provide connectivity and stability to merge board, ESC holders, control board and power conversion board.
  + Takes in 14.8V at 40A from current merge circuit.
  + Delivers 5V, 12V, 19V, and 48V from the power conversion board to the controls system, CPU, and sensors.
  + Provide PWM from the controls system to ESCs.

